**New, clean break temperature control range**

The new clean break HASCO temperature control program offers users maximum safety during uncoupling. It impresses with its excellent tightness and durability.

**Safe and reliable coupling of cooling lines**

The innovative temperature control system with flat end sealing surfaces and shuts offs on both sides enables clean break opening and closing under pressure without media leakage.

The one-handed quick-release couplings with a particularly long and precise guidance for the sealing nipple and guarantee safe and independent coupling with a maximum flow rate and only a low pressure drop.

The High-quality materials 2.0401 (brass) and 1.4305 (stainless steel) make the quick-release couplings robust against vibrations and movements. The stainless-steel versions are ideal for use in medical and cleanroom-technology applications.

The couplings are also suitable for high-temperature applications as a function of the cooling medium. They guarantee a reliable and long-lasting production process and round off the extensive HASCO temperature-control program.

10/2020