**Extension to range of control units H1250/…**

With an addition to its range of control units H1250/… Basezone, HASCO hot runner has extended its hot runner product portfolio. In addition to the two devices with one and two control zones, a unit with four control zones is now also immediately available.

**Rugged control units boast outstanding simplicity**

The rugged control unit range H1250/… stands out through its simplicity. It is designed as a plug-and-play unit and dispenses with extended features. It only has the classic additional features such as boost and standby function as well as a switch-over option to manual mode in percent.

**Intuitive operation and precise control**

The unit is operated via a clearly arranged, self-explanatory membrane keypad, in each case directly next to the temperature display. For each zone, corresponding control displays transmit the current status and unambiguous error reports such as a sensor break or excess temperature.

**New compact 4-zone device immediately available ex stock**

The new 4-zone device is very compact in design with a width of 210 mm and a height of 175 mm, and can thus be simply positioned next to the injection moulding machine. As with the previous units, the new 4-zone control unit is immediately available ex stock at a very attractive price.

04/2021