**New: Cycle counter A57300/… for optimum process data monitoring**

The new HASCO mechanical cycle counter A57300/... marks a further addition to the HASCO counter range and is used wherever there is a need to monitor process data.

With the actuator pin on the left, the counter offers mounting many options. The cycle counter can be installed on either the fixed half or the moving half (non operator side) of the mould. It has a 7-digit, mechanical, non-resettable counter, can be mounted easily and rapidly, is completely maintenance-free and does not require a power supply.

The cycle counter A57300/… can be used at an ambient temperature

of up to 120°C. Safe and reliable counting during the entire injection moulding process ensures optimum process data monitoring.

07/2020