**HASCO Extended tube reduction Z906/...**

Connection threads for mould cooling systems are frequently located at deeper points on injection moulds. HASCO supplies special extended tubes for achieving an optimum connection between the hoses and the temperature control unit.

**Now available with inch threads too**

The extended tube reduction Z906/... is now also available in the standard inch sizes. Made of quality material 2.0401, the component ensures a maximum flow rate. It guarantees a reliable, long service life and helps boost process reliability. Available for systems 9 and 13, the extended tube reduction provides simple, functional and reliable connections.

12/2020